**OPTICAL TERMINATION CLOSURE**

**Scope of delivery**

* seals and cassettes pre-fabricated and equipped according customer requirements
* pre-fabricated tube / hose packages according customer requirements
* pressure valve
* RFID Chip / BAR-Code / QR-Code
* grounding kit
* additional internal strain relief
* additional outer cable clamp
* splitter
* Options:

**Material**

plastic, aluminum

**Dimensions**

height 600 mm, diameter 300 mm

**Article Code**

2LINE OTC

Brand: ZweiCom-Hauff GmbH

**Hauff-Technik GRIDCOM GmbH**

**Manufacturer information**

Hauff-Technik GRIDCOM GmbH

Geiselroter Heidle 1

73494 Rosenberg, GERMANY

Telefon +49 79 67 90 08 - 30

Fax +49 79 67 90 08 - 99